<h1 align = "center">🌟LILYGO T-keyboard🌟</h1>

## **English | [中文](./README_CN.MD)**



<h3 align = "left">Quick start:</h3>

**USE Arduino IDE**

1. Install the current upstream Arduino IDE at the 1.8 level or later. The current version is at the [Arduino website](http://www.arduino.cc/en/main/software).
2. Start Arduino and open Preferences window. In additional board manager add url: https://raw.githubusercontent.com/espressif/arduino-esp32/gh-pages/package_esp32_index.json .separating them with commas.
3. Select Tools -> Board -> ESP32C3 Dev Module
4. If you do not have a driver installed, you need to install it (Window:ch341ser2.exe, MAC:ch34x_mac_driver_v1.6.zip [New driver reference](https://github.com/LilyGO/LILYGO-T-OI/issues/3#issuecomment-907645945 ))
5. Need to install the following dependencies
     - [ESP32-BLE-Keyboard](https://github.com/T-vK/ESP32-BLE-Keyboard/tree/0.3.0)
     - [T-0.99TFT](https://github.com/Xinyuan-LilyGO/T-0.99TFT)



<h3 align = "left">Product 📷:</h3>

|  Product   | Product  Link  |
| :--------: | :------------: |
| T-keyboard | [AliExpress]() |

## Pinout

![](image/)








